# Details of Ghostscript output devices

## Table of contents

> - Notes on measurements
> - Image file formats
>   - PNG file format
>   - JPEG file format (JFIF)
>   - PNM file format
>   - TIFF file formats
>   - fax file formats
>   - BMP file format
>   - PCX file format
>   - PSD file format (DeviceN color model)
> - High level formats
>   - PDF file output
>   - PostScript file output
>   - EPS file output
>   - PCL-XL file output
> - Display devices
>   - X Window System
>   - display device (MS Windows, OS/2, gtk+)
> - IJS - Inkjet and other raster devices
> - Rinkj - Resplendent inkjet driver
> - HP Deskjet official drivers
> - Gimp-Print driver collection
> - MS Windows printers
> - Sun SPARCprinter
>   - Installation
>   - Problems
> - Apple dot matrix printer
> - Test devices
>   - Permutation (DeviceN color model)
>   - spotcmyk (DeviceN color model)
>   - XCF (DeviceN color model)
>   - Raw 'bit' devices

For other information, see the Ghostscript overview. You may also be interested in how to build Ghostscript and install it, as well as the description of the driver interface.

Documentation for some older, superceded devices has been moved to another document. In general such devices are deprecated and will be removed in future versions of Ghostscript. In general all older printer drivers can be replaced by the ijs interface and one of the available 3rd party raster driver collections. We recommend moving to the ijs device for all such printing.

## Notes on measurements

Several different important kinds of measures appear throughout this document: inches, centimeters and millimeters, points, and bits per pixel.

Centimeters and millimeters
  ISO standard paper sizes such as A4 and A3 are commonly represented in the SI units of centimeters and millimeters. Centimeters are abbreviated cm, millimeters mm. ISO A4 paper is quite close to 210×297 millimeters (approximately 8.3×11.7 inches).
Inches
  1 inch equals 2.54 centimeters. The inch measure is sometimes represented by in or a quotation mark (") to the right of a measure, like 8.5in or 8.5". U.S. "letter" paper is exactly 8.5in×11in, approximately 21.6cm×27.9cm. (See in the usage documentation all the paper sizes predefined in Ghostscript.)
Points
  Points are a measure traditionally used in the printing trade and now in PostScript, which specifies exactly 72 points per inch (approximately 28.35 per centimeter). The paper sizes known to Ghostscript are defined in the initialization file `gs_statd.ps` in terms of points.
Dots per inch
  Dots per inch or dpi is the common measure of printing resolution in the US.
Bits per pixel
  Commonly abbreviated bpp this is the number of digital bits used to represent the color of each pixel. This is also referred to as 'bit depth' or 'pixel depth'.

## Image file formats

Ghostscript supports output to a variety of image file formats and is widely used for rasterizing postscript and pdf files. A collection of such formats ('output devices' in Ghostscript terminology) are described in this section.

Here are some commonly useful driver options that apply to all raster drivers. Options specific to particular file formats are described in their respective sections below.

> -sOutputFile=filename

>   This is a general option telling Ghostscript what to name the output. It can either be a single filename '`tiger.png`' or a template '`figure-%03d.jpg`' where the `%03d` is replaced by the page number.

> -rres
> -rxresxyres

>   This option sets the resolution of the output file in dots per inch. The default value if you don't specify this options is usually 72 dpi.

> -dTextAlphaBits=n
> -dGraphicsAlphaBits=n

>   These options control the use of subsample antialiasing. Their use is highly recommended for producing high quality rasterizations of the input files. The size of the subsampling box n should be 4 for optimum output, but smaller values can be used for faster rendering. Antialiasing is enabled separately for text and graphics content.

It is also conventional to call Ghostscript with the '`-dSAFER -dBATCH -dNOPAUSE`' trio of options when rasterizing to a file. These suppress interactive prompts and enable some security checks on the file to be run. Please see the Use documentation for a complete description.

### PNG file format

PNG (pronounced 'ping') stands for Portable Network Graphics, and is the recommended format for high-quality images. It supports full quality color and transparency, offers excellent lossless compression of the image data, and is widely supported. Please see the PNG website for a complete description of the format.

Ghostscript provides a variety of devices for PNG output varying by bit depth. For normal use we recommend `png16m` for 24-bit RGB color, or `pnggray` for grayscale. The png256, png16 and pngmono devices respectively provide 8-bit color, 4-bit color and black-and-white for special needs.

The pngalpha device is 32-bit RGBA color with transparency indicating pixel coverage. The background is transparent unless it has been explicitly filled. PDF 1.4 transparent files do not give a transparent background with this device. Text and graphics anti-aliasing are enabled by default.

#### Options

The pngalpha device has one option. The other png devices have no special options.

> `-dBackgroundColor=`16#RRGGBB (RGB color, default white = 16#ffffff)
>   For the `pngalpha` device only, set the suggested background color in the PNG bKGD chunk. When a program reading a PNG file does not support alpha transparency, the PNG library converts the image using either a background color if supplied by the program or the bKGD chunk. One common web browser has this problem, so when using `<body bgcolor="CCCC00">` on a web page you would need to use `-dBackgroundColor=16#CCCC00` when creating alpha transparent PNG images for use on the page.

#### Examples

Examples of how to use Ghostscript to convert postscript to PNG image files:

>      gs -dSAFER -dBATCH -dNOPAUSE -sDEVICE=png16m -dGraphicsAlphaBits=4 \
>           -sOutputFile=tiger.png examples/tiger.png

>      gs -dSAFER -dBATCH -dNOPAUSE -r150 -sDEVICE=pnggray -dTextAlphaBits=4 \
>           -sOutputFile=doc-%02d.png doc.pdf

### JPEG file format (JFIF)

Ghostscript includes output drivers that can produce jpeg files from postscript or pdf images. These are the `jpeg` and `jpeggray` devices.

Technically these produce Independent JPEG Group JFIF (JPEG File Interchange Format) files, the common sort found on the web.

Please note that JPEG is a compression method specifically intended for continuous-tone images such as photographs, not for graphics, and it is therefore quite unsuitable for the vast majority of page images produced with PostScript. For anything other than pages containing simple images the lossy compression of the jpeg format will result in poor quality output regardless of the input. To learn more about the distinction, consult a reference about uses and abuses of JPEG, such as the JPEG FAQ

> http://www.faqs.org/faqs/jpeg-faq/

#### Examples

You can use the JPEG output drivers -- `jpeg` to produce color JPEG files and `jpeggray` for grayscale JPEGs -- the same as other file-format drivers: by specifying the device name and an output file name, for example

>     gs -sDEVICE=jpeg -sOutputFile=foo.jpg foo.ps

#### Options

The JPEG devices support several special parameters to control the JPEG "quality setting" (DCT quantization level).

> `-dJPEGQ=`N (integer from 0 to 100, default 75)
>   Set the quality level N according to the widely used IJG quality scale, which balances the extent of compression against the fidelity of the image when reconstituted. Lower values drop more information from the image to achieve higher compression, and therefore have lower quality when reconstituted.
> `-dQFactor=`M (float from 0.0 to 1.0)
>   Adobe's QFactor quality scale, which you may use in place of `JPEGQ` above. The QFactor scale is used by PostScript's DCTEncode filter but is nearly unheard-of elsewhere.

At this writing the default JPEG quality level of 75 is equivalent to `-dQFactor=0.5`, but the JPEG default might change in the future. There is currently no support for any additional JPEG compression options, such as the other DCTEncode filter parameters.

### PNM

The PNM (portable network map) family of formats are very simple uncompressed image formats commonly used on unix-like systems. They are particularly useful for testing or as input to an external conversion utility.

A wide variety of data formats and depths is supported. Devices include `pbm pbmraw pgm pgmraw pgnm pgnmraw pnm pnmraw ppm ppmraw pkm pkmraw pksm pksmraw`.

### TIFF file formats

TIFF is a loose collection of formats, now largely superceded by PNG except in applications where backward compatibility or special compression is required. The TIFF file format is described in the TIFF 6.0 Specification published by Adobe Systems Incorporated.

There are two unrelated sets of TIFF drivers. There are five color TIFF drivers that produce uncompressed output:

> `tiffgray`
>   Produces 8-bit gray output.
> `tiff12nc`
>   Produces 12-bit RGB output (4 bits per component).
> `tiff24nc`
>   Produces 24-bit RGB output (8 bits per component).
> `tiff32nc`
>   Produces 32-bit CMYK output (8 bits per component).
> `tiffsep`
>   The tiffsep device creates multiple output files. The device creates a single 32 bit composite CMYK file (tiff32nc format) and multiple tiffgray files. A tiffgray file is created for each separation.

>   The file specified via the OutputFile command line parameter will contain CMYK data. This data is based upon the CMYK data within the file plus an equivalent CMYK color for each spot colors which is present. The equivalent CMYK color for each spot colors is determined using the alternate tint transform function specified in Separation and DeviceN color spaces. Since this file is created based upon having color planes for each colorant, the file will correctly represent the appearance of overprinting with spot colors.

>   File names for the separations for the CMYK colorants are created by appending '.Cyan.tif', '.Magenta.tif' '.Yellow.tif' or '.Black.tif' to the to the end of the file name specified via the OutputFile parameter. File names for the spot color separation files are created by appending '.sn.tif' (where n is the spot color number, see below) to the end of the file name specified via the OutputFile parameter. (If the file name specified via the OutputFile parameter ends with the suffix '.tif', then the suffix is removed prior to adding 'Cyan.tif', etc.)

>   The tiffsep device will automatically recognize spot colors. In this case their order is determined by when they are found in the input file. The names of spot colors may be specified via the SeparationColorNames device parameters.

>   Internally each spot color is assigned a spot color number. These numbers start with 0 for the first spot color. The spot color numbers are assigned in the same order as the names are printed to stderr (see below). This order also matches the ordering in the SeparationColorNames list, if this parameter is specified. The spot color numbers are not affected by the SeparationOrder parameter.

>   If only a subset of the colorants for a file is desired then the separations to be output can be selected via the SeparationOrder device parameter. When colorants are selected via the SeparationOrder parameter, the composite CMYK output contains the equivalent CMYK data only for the selected colorants.

>   The tiffsep device also prints the names of any spot colors detected within a document to stderr. (stderr is also used for the output from the bbox device.) For each spot color the name of the color is printed preceded by '%%SeparationName: '. This provides a simple mechanism for users and external applications to be informed about the names of spot colors with a document.

>   Generally Ghostscript will support a maximum of 64 process and spot colors. However the maximum may be smaller if the C compiler that was used to build Ghostscript does not support a 64 bit integer type. MSVC, gcc, and most current compilers do support a 64 integer type. For those compilers that have 32 bits as the largest integer type, then only 4 separations can be produced per Ghostscript pass. However it is possible to handle more than 4 colorants by doing multiple passes. For each pass after the first one, the names of all of the separations need to be specified via the SeparationColorNames parameter and the names of the desired separations need to be specified via the SeparationOrder parameter. For instance, add the following to the command line: `-c "<< /SeparationColorNames [ /Name1 /Name2 ] /SeparationOrder [ /Name1 ] >> setpagedevice" -f`. This will produce a single separation file for the spot color called 'Name1'. It is possible to create an overall CMYK composite for more than 4 colorants by then adding together (via an external application like imagemagick) the composite CMYK output files from the individual Ghostscript passes.

The remaining TIFF drivers all produce black-and-white output with different compression modes:

> `tiffcrle`
>   G3 fax encoding with no EOLs
> `tiffg3`
>   G3 fax encoding with EOLs
> `tiffg32d`
>   2-D G3 fax encoding
> `tiffg4`
>   G4 fax encoding
> `tifflzw`
>   LZW-compatible (tag = 5) compression
> `tiffpack`
>   PackBits (tag = 32773) compression

#### Options

The black-and-white TIFF drivers support creation of files that are comprised of more than a single strip. Multi-strip files reduce the memory requirement on the reader, since readers need only store and process one strip at a time. These drivers provide two parameters beyond the standard set:

> `-dMaxStripSize=`N (non-negative integer; default = 0)
>   Set the maximum (uncompressed) size of a strip.
> `-dAdjustWidth=`state (0 or 1; default = 1)
>   If this option set then if the requested page width is in the range of either 1680..1736 or 2000..2056 columns, set the page width to A4 (1728 columns) or B4 (2048 columns) respectively. This behavior is the default. Pass -dAdjustWidth=0 to turn off this behavior.

The TIFF 6.0 specification, Section 7, page 27, recommends that the size of each strip be about 8 Kbytes. As an example, to generate the 'tiger' in tiffg4 format that has the recommended strip size, use:

>     gs -sDEVICE=tiffg4 -sOutputFile=tiger.tiff -dMaxStripSize=8192 examples/tiger.eps

If the value of the `MaxStripSize` parameter is smaller than a single image row, then no error will be generated, and the TIFF file will be generated correctly using one row per strip. Note that smaller strip sizes increase the size of the file by increasing the size of the StripOffsets and StripByteCounts tables, and by reducing the effectiveness of the compression which must start over for each strip.

If the value of MaxStripSize is 0 (the default), then the entire image will be a single strip.

Since v. 8.51 the logical order of bits within a byte, FillOrder, tag = 266 is controlled by a parameter:

> `-dFillOrder=`1 | 2 (default = 1)
>   If this option set to 2 then pixels are arranged within a byte such that pixels with lower column values are stored in the lower-order bits of the byte; otherwise pixels are arranged in reverse order.

Earlier versions of Ghostscript always generated TIFF files with FillOrder = 2. According to the TIFF 6.0 specification, Section 8, page 32, support of FillOrder = 2 is not required in a Baseline TIFF compliant reader

### FAX

Ghostscript supports a variety of fax encodings, both encapsulated in TIFF (see above) and as raw files. The later case is described here.

The fax devices are `faxg3`, `faxg32d` and `faxg4`.

### BMP

BMP is a simple uncompressed image format commonly used on MS Windows. It is supported by the devices `bmpmono bmpgray bmpsep1 bmpsep8 bmp16 bmp256 bmp16m bmp32b`.

### PCX

PCX is an image format sometimes used on MS Windows. It has some support for image compression and alternate color spaces, and so can be a useful way to output CMYK. It is supported by the `pcxmono pcxgray pcx16 pcx256 pcx24b pcxcmyk` series of devices.

### PSD

PSD is the image format used by Adobe Photoshop. It is supported by the `psdcmyk` and `psdrgb` devices. Of special interest with the `psdcmyk` device is that it supports spot colors. See the comments under the tiffsep device about the maximum number of spot colors supported by Ghostscript

## High-level devices

In addition to raster image files, Ghostscript supports output in a number of 'high-level' formats. These allow Ghostscript to preserve (as much as possible) the drawing elements of the input file maintaining flexibility, resolution independence, and editability.

### PDF writer

The `pdfwrite` device outputs PDF. Please refer to Ps2pdf.htm for the extensive `pdfwrite` device options.

### PS writer

The `pswrite` device outputs postscript.

#### Options

> `-dLanguageLevel=`1 | 1.5 | 2 | 3 (default is 2)
>   Set the language level of the generated file. Language level 1.5 is language level 1 with color extensions. Currently language level 3 generates the same PostScript as 2.

### EPS writer

The `epswrite` device outputs encapsulated postscript.

#### Options

> `-dLanguageLevel=`1 | 1.5 | 2 | 3 (default is 2)
>   Set the language level of the generated file. Language level 1.5 is language level 1 with color extensions. Currently language level 3 generates the same PostScript as 2.

### PXL

The `pxlmono` and `pxlcolor` devices output HP PCL-XL, a graphic language understood by many recent laser printers.

## Display Devices

Ghostscript is often used for screen display of postscript and pdf documents. In many cases, a client or 'viewer' application calls the Ghostscript engine to do the rasterization and handles the display of the resulting image itself, but it is also possible to invoke Ghostscript directly and select an output device which directly handles displaying the image on screen.

This section describes the various display-oriented devices that are available in Ghostscript.

### X Window System

Perhaps the most common use of of a display device is with the X Window System on unix-like systems. It is the default device on the command line client on such systems, and is used more creatively by the gv client application.

The available devices are:

x11
  This is the default device, handling display on X11R6.
x11alpha
  This is the x11 device, but with antialiasing. It is equivalent to invoking the x11 device with the options `-dGraphicsAlphaBits=4 -dTextAlphaBits=4 -dMaxBitmap=50000000`.
x11cmyk
  This device rasterizes the image in the CMYK color space, then flattens it to RGB for display. It's intended for testing only.
x11mono
  This is a strict black-and-white device for 1-bit monochrome displays.
x11gray2
  This is a device for 2 bpp (4-level) monochrome displays.
x11gray4
  This is a device for 4 bpp (16-level) monochrome displays.

### display device (MS Windows, OS/2, gtk+)

The `display` device is used by the MS Windows, OS/2 and the gtk+ versions of ghostscript.

#### Options

The display device has several user settable options.

> `-dDisplayFormat=`N (integer bit-field)
>   Some common values are 16#30804 for Windows RGB, 16#804 for gtk+ RGB, 16#20101 for Windows monochrome, 16#102 for gtk+ monochrome, 16#20802 grayscale, 16#20808 for CMYK, 16#a0800 for separations. The bit fields are
>   - native (1), gray (2), RGB (4), CMYK (8), or separation (80000) color spaces.
>   - unused first byte (40) or last byte (80).
>   - 1 (100), 4 (400), or 8 (800) bits/component.
>   - bigendian (00000 = RGB) or littleendian (10000 = BGR) order.
>   - top first (20000) or bottom first (00000) raster.
>   - 16 bits/pixel with 555 (00000) or 565 (40000) bitfields.
>   For more details, see the Ghostscript Interpreter API.
> `-dDisplayResolution=`DPI
>   Set the initial resolution resolution for the display device. This is used by the Windows clients to set the display device resolution to the Windows display logical resolution. This can be overriden by the command line option `-r` DPI.

When using the separation color space, the following options may be set using setpagedevice, as described in the PostScript Language Reference:

> `SeparationColorNames`
>   An array giving the names of the spot colors
> `SeparationOrder`
>   An array giving the names and order of the colorants to be output.

## IJS - Inkjet and other raster devices

IJS is a relatively new initiative to improve the quality and ease of use of inkjet printing with Ghostscript. Using IJS, you can add new drivers, or upgrade existing ones, without recompiling Ghostscript. All driver authors are encouraged to adapt their drivers for IJS, and if there is an IJS driver available for your printer, it should be your first choice.

Please see the IJS web page for more information about IJS, including a listing of IJS-compatible drivers.

A typical command line for IJS is:

> `gs -dSAFER -sDEVICE=ijs -sIjsServer=hpijs -sDeviceManufacturer=HEWLETT-PACKARD -sDeviceModel='DESKJET 990' -dIjsUseOutputFD -sOutputFile=/dev/usb/lp1 -dNOPAUSE -- examples/tiger.eps`

Individual IJS command line parameters are as follows:

`-sIjsServer=`{path}
  Sets the pathname for the IJS server (ie printer driver). Ghostscript will spawn a new process for this driver, and communicate with it using the IJS protocol. The pathname need not be absolute, as the PATH environment variable is searched, but it's probably a good idea for robustness and security. Note also that if -dSAFER is not specified, it's possible for PostScript code to set this parameter, so it can cause arbitrary code to be executed. See the section on Security for more information.

`-sDeviceManufacturer=`{name}
`-sDeviceModel=`{name}
  These parameters select the device according to IEEE-1284 standard device ID strings. In general, consult the documentation for the driver to find the appropriate settings. Note that, if the value contains a space, you'll want to quote the value in your shell, as in the example above.

`-sIjsParams=`{params}
  This parameter allows you to set arbitrary IJS parameters on the IJS driver. The format is a comma-separated list of `key=value` pairs. If it is necessary to send a value containing a comma or backslash, it can be escaped with a backslash. Thus, `'-sIjsParams=Foo=bar,Baz=a\,b'` sets the parameter Foo to "bar", and Baz to "a,b".

`-dIjsUseOutputFD`
  This flag indicates that Ghostscript should open the output file and pass a file descriptor to the server. If not set, Ghostscript simply passes the filename set in OutputFile to the server. In most cases, this flag won't matter, but if you have a driver which works only with OutputFD (such as hpijs 1.0.2), or if you're using the -sOutputFile="|cmd" syntax, you'll need to set it.

`-dBitsPerSample=`N
  This parameter controls the number of bits per sample. The default value of 8 should be appropriate for most work. For monochrome images, use -dBitsPerSample=1.

Generic Ghostscript options that are particularly relevant for IJS are summarized below:

`-r` number
`-r` number1 `x` number2
  Sets the resolution, in dpi. If the resolution is not specified, Ghostscript queries the IJS server to determine the preferred resolution. When the resolution is specified, it overrides the value (if any) preferred by the IJS server.

`-dDuplex`
`-dTumble`
  These flags enable duplex (two-sided) printing. Tumble controls the orientation. When Tumble is false, the pages are oriented suitably at the left or right. When Tumble is true, the pages are oriented suitably for binding at the top or bottom.

`-sProcessColorModel=`{name}
  Use this flag to select the process color model. Suitable values include DeviceGray, DeviceRGB, and DeviceCMYK.

### Building IJS

IJS is included by default on Unix gcc builds, and also in autoconf'ed builds. Others may need some makefile tweaking. First, make sure the IJS device is selected:

> DEVICE_DEVS2=$(DD)ijs.dev

Next, make sure that the path and execution type are set in the top level makefile. The values for Unix are as follows:

> IJSSRCDIR=ijs IJSEXECTYPE=unix

At present, "unix" and "win" are the only supported values for IJSEXECTYPE. If neither sounds appropriate for your system, it's possible that more porting work is needed.

Last, make sure that ijs.mak is included in the top level makefile. It should be present right after the include of icclib.mak.

IJS is not inherently platform-specific. We're very much interested in taking patches from people who have ported it to non-mainstream platforms. And once it's built, you won't have to recompile Ghostscript to support new drivers!

## Rinkj - Resplendent inkjet driver

The Rinkj driver is an experimental new driver, capable of driving some Epson printers at a very high level of quality. It is not currently recommended for the faint of heart.

You will need to add the following line to your makefile:

> DEVICE_DEVS2=$(DD)rinkj.dev

Most of the configuration parameters, including resolution, choice of printer model, and linearization curves, are in a separate setup file. In addition, we rely heavily on an ICC profile for mapping document colors to actual device colors.

A typical command line invocation is:

> `gs -r1440x720 -sDEVICE=rinkj -sOutputFile=/dev/usb/lp0 -sSetupFile=lib/rinkj-2200-setup -sProfileOut=2200-cmyk.icm -dNOPAUSE -dBATCH file.ps`

Individual Rinkj command line parameters are as follows:

`-sSetupFile=`{path}
  Specifies the path for the setup file.
`-sProfileOut=`{path}
  Specifies the path for the output ICC profile. This profile should be a link profile, mapping the ProcessColorModel (DeviceCMYK by default) to the device color space.

For 6- and 7-color devices, the target color space for the output profile is currently a 4-component space. The conversion from this into the 6- or 7-color space (the "ink split") is done by lookup tables in the setup file.

Setup files are in a simple "Key: value" text format. Relevant keys are:

`Manufacturer:`{name}
`Model:`{name}
  The manufacturer and model of the individual device, using the same syntax as IEEE printer identification strings. Currently, the only supported manufacturer string is "EPSON", and the only supported model strings are "Stylus Photo 2200" and "Stylus Photo 7600".
`Resolution:`{x-dpi}x{y-dpi}
  The resolution in dpi. Usually, this should match the Ghostscript resolution set with the `-r` switch. Otherwise, the page image will be scaled.
`Dither:`{int}
  Selects among variant dither options. Currently, the choices are `1` for one-bit dither, and `2`, for a 2-bit variable dot dither.
`Aspect:`{int}
  Controls the aspect ratio for highlight dot placement. Valid values are `1`, `2`, and `4`. For best results, choose a value near the x resolution divided by the y resolution. For example, if resolution is 1440x720, aspect should be 2.
`Microdot:`{int}
  Chooses a microdot size. On EPSON devices, this value is passed directly through to the "ESC ( e" command. See EPSON documentation for further details (see, I told you this wasn't for the faint of heart).
`Unidirectional:`{int}
  Enables (1) or disables (0) unidirectional printing, which is slower but possibly higher quality.
`AddLut:`{plane}
  Adds a linearization look-up table. The plane is one of "CcMmYKk". The lookup table data follows. The line immediately following AddLut is the number of data points. Then, for each data point is a line consisting of two space-separated floats - the output value and the input value. If more than one LUT is specified for a single plane, they are applied in sequence.

A typical setup file is supplied in `lib/rinkj-2200-setup`. It is configured for the 2200, but can be adapted to the 7600 just by changing the "Model" line.

In addition, sample profiles are available at artofcode.com/rinkj/profiles/.

A known issue with this driver is poor support for margins and page size. In some cases, this will cause an additional page to be ejected at the end of a job. You may be able to work around this by supplying a cut-down value for `-dDEVICEHEIGHTPOINTS`, for example 755 for an 8.5x11 inch page on the EPSON 2200.

## HP Deskjet official drivers

HP provides official drivers for many of their Deskjet printer models. In order to use these drivers, you will need the HP Inkjet Server as well as Ghostscript, available from http://hpinkjet.sourceforge.net. This version of Ghostscript includes the patch from version 0.97 of the hpijs software. If you are installing hpijs from an RPM, you will only need the hpijs RPM, not the Ghostscript-hpijs one, as the code needed to work with hpijs is already included.

Note that newer version of the hpijs drivers support the IJS protocol. If you can, you should consider using the ijs driver instead. Among other things, the hpijs Ghostscript driver is Unix-only, and is untested on older Unix platforms.

As of the 0.97 version, hpijs supports the following printer models:

e-Series:
  e-20
DeskJet 350C Series:
  350C
DeskJet 600C Series:
  600C, 660C, 670/672C, 670TV, 680/682C
DeskJet 600C Series Photo:
  610/612C, 640/648C, 690/692/693/694/695/697C
DeskJet 630C Series:
  630/632C
DeskJet 800C Series:
  810/812C, 830/832C, 840/842/843C, 880/882C, 895C
DeskJet 900C Series, PhotoSmart::
  930/932C, 950/952C, 970C, PhotoSmart 1000/1100
DeskJet 990C, PhotoSmart:
  960C, 980C, 990C, PhotoSmart 1215/1218

You will need to add the following line to your makefile:

> DEVICE_DEVS2=$(DD)DJ630.dev $(DD)DJ6xx.dev $(DD)DJ6xxP.dev $(DD)DJ8xx.dev $(DD)DJ9xx.dev $(DD)DJ9xxVIP.dev $(DD)AP21xx.dev

Please see http://hpinkjet.sourceforge.net for more information about this driver. Thanks to the folks at HP, especially David Suffield for making this driver available and working to integrate it with Ghostscript.

## Gimp-Print driver collection

The Gimp-Print project provides a large collection of printer drivers with an IJS interface. Please see their website for details.

## MS Windows printers

This section was written by Russell Lang, the author of Ghostscript's MS Windows-specific printer driver, and updated by Pierre Arnaud, the current maintainer.

The `mswinpr2` device uses MS Windows printer drivers, and thus should work with any printer with device-independent bitmap (DIB) raster capabilities. The printer resolution cannot be selected directly using PostScript commands from Ghostscript: use the printer setup in the Control Panel instead. It is however possible to specify a maximum resolution for the printed document (see below).

If no Windows printer name is specified in `-sOutputFile`, Ghostscript prompts for a Windows printer using the standard Print Setup dialog box. You must set the orientation to Portrait and the page size to that expected by Ghostscript; otherwise the image will be clipped. Ghostscript sets the physical device size to that of the Windows printer driver, but it does not update the PostScript clipping path.

If a Windows printer name is specified in `-sOutputFile` using the format `"%printer%printer_name"`, for instance

> `gs ... -sOutputFile="%printer%Apple LaserWriter II NT"`

then Ghostscript attempts to open the Windows printer without prompting (except, of course, if the printer is connected to `FILE:`). Ghostscript attempts to set the Windows printer page size and orientation to match that expected by Ghostscript, but doesn't always succeed. It uses this algorithm:

1. If the requested page size matches one of the Windows standard page sizes +/- 2mm, request that standard size.
2. Otherwise if the requested page size matches one of the Windows standard page sizes in landscape mode, ask for that standard size in landscape.
3. Otherwise ask for the page size by specifying only its dimensions.
4. Merge the requests above with the defaults. If the printer driver ignores the requested paper size, no error is generated: it will print on the wrong paper size.
5. Open the Windows printer with the merged orientation and size.

The Ghostscript physical device size is updated to match the Windows printer physical device.

### Supported command-line parameters

The `mswinpr2` device supports a limited number of command-line parameters (e.g. it does not support setting the printer resolution). The recognized parameters are the following:

> `-sDEVICE=mswinpr2`
>   Selects the MS Windows printer device. If Ghostscript was not compiled with this device as the default output device, you have to specify it on the command line.
> `-dNoCancel`
>   Hides the progress dialog, which shows the percent of the document page already processed and also provides a cancel button. This option is useful if GS is intended to print pages in the background, without any user intervention.
> `-sOutputFile=`"%printer%printer_name"
>   Specifies which printer should be used. The printer_name should be typed exactly as it appears in the Printers control panel, including spaces.

### Supported options (device properties)

Several extra options exist which cannot be set through the command-line, but only by executing the appropriate PostScript setup code. These options can be set through the inclusion of a setup file on the command-line:

> `gs ... setup.ps ...`

The `setup.ps` file is responsible for the device selection, therefore you should not specify the `-sDEVICE=mswinpr2` option on the command-line if you are using such a setup file. Here is an example of such a setup file:

>     mark
>       /NoCancel      true                       % don't show the cancel dialog
>       /BitsPerPixel  4                          % force 4 bits/pixel
>       /UserSettings
>         <<
>           /DocumentName  (Ghostscript document) % name for the Windows spooler
>           /MaxResolution 360                    % maximum document resolution
>         >>
>       (mswinpr2) finddevice                     % select the Windows device driver
>       putdeviceprops
>     setdevice

This example disables the progress dialog (same as the `-dNoCancel` option), forces a 4 bits/pixel output resolution and specifies additional user settings, such as the document name (which will be displayed by the Windows spooler for the queued document) and the maximum resolution (here 360 dpi). It then finds and selects an instance of the MS Windows device printer and activates it. This will show the standard printer dialog, since no `/OutputFile` property was specified.

The following options are available:

> `/NoCancel boolean`
>   Disables (hides) the progress dialog when set to `true` or show the progress dialog if not set or set to `false`.
> `/OutputFile string`
>   Specifies which printer should be used. The string should be of the form `%printer%printer_name`, where the printer_name should be typed exactly as it appears in the Printers control panel, including spaces.
> `/QueryUser integer`
>   Shows the standard printer dialog (`1` or any other value), shows the printer setup dialog (`2`) or selects the default Windows printer without any user interaction (`3`).
> `/BitsPerPixel integer`
>   Sets the device depth to the specified bits per pixel. Currently supported values are `1` (monochrome), `4` (CMYK with screening handled by Ghostscript) and `24` (True Color, dithering handled by the Windows printer driver; this option can produce huge print jobs).
> `/UserSettings dict`
>   Sets additional options, defined in a dictionary. The following properties can be set:
>   `/DocumentName string`
>     Defines the user friendly document name which will be displayed by the Windows spooler.
>   `/DocumentRange [n1 n2]`
>     Defines the range of pages contained in the document. This information can be used by the printer dialog, in conjunction with the following property.
>   `/SelectedRange [n1 n2]`
>     Defines the selected range of pages. This information will be displayed in the printer dialog and will be updated after the user interaction. A PostScript program could check these values and print only the selected page range.
>   `/MaxResolution dpi`
>     Specifies the maximum tolerated output resolution. If the selected printer has a higher resolution than `dpi`, then Ghostscript will render the document with a submultiple of the printer resolution. For example, if `MaxResolution` is set to 360 and the output printer supports up to 1200 dpi, then Ghostscript renders the document with an internal resolution of 1200/4=300 dpi. This can be very useful to reduce the memory requirements when printing in True Color on some high resolution ink-jet color printers.

These properties can be queried through the `currentpagedevice` operator. The following PostScript code snippet shows how to do it for some of the properties:

>     currentpagedevice /BitsPerPixel get ==  % displays the selected depth

>     currentpagedevice /UserSettings get     % get the additional options..
>     /us exch def                            % ..and assign them to a variable

>     us /DocumentName get ==     % displays the document name
>     us /SelectedRange get ==    % displays the selected page range

>     % other misc. information (don't rely on them)

>     us /Color get ==            % 1 => monochrome output, 2 => color output
>     us /PrintCopies get ==      % displays the number of copies requested

There are a few undocumented parameters stored in the `UserSettings` dictionary. You should not rely on them. Their use is still experimental and they could be removed in a future version.

### Duplex printing

If the Windows printer supports the duplex printing feature, then it will also be available through the `mswinpr2` device. You can query for this support through the `/Duplex` property of the `currentpagedevice`. If it returns `null`, then the feature is not supported by the selected printer. Otherwise, `true` means that the printer is currently set up to print on both faces of the paper and `false` that it is not, but that it can.

The following example shows how to print on both faces of the paper (using the long side of the paper as the reference):

>     << /Duplex true /Tumble false >> setpagedevice

## Sun SPARCprinter

This section was contributed by Martin Schulte.

With a SPARCprinter you always buy software that enables you to do PostScript printing on it. A page image is composed on the host, which sends a bitmap to the SPARCprinter through a special SBUS video interface. So the need for a Ghostscript interface to the SPARCPrinter seems low, but on the other hand, Sun's software prints some PostScript drawings incorrectly: some pages contain a thin vertical line of rubbish, and on some Mathematica drawings the text at the axes isn't rotated. Ghostscript, however, gives the correct results. Moreover, replacing proprietary software should never be a bad idea.

The problem is that there has yet been no effort to make the SPARCPrinter driver behave like a BSD output filter. I made my tests using the script shown here.

### Installation

Add `sparc.dev` to `DEVICE_DEVS` and compile Ghostscript as described in the documentation on how to build Ghostscript. Afterwards you can use the following script as an example for printing after modifying it with the right pathnames -- including for {GSPATH} the full pathname of the Ghostscript executable:

>     outcmd1='/vol/local/lib/troff2/psxlate -r'
>     outcmd2='{GSPATH} -sDEVICE=sparc -sOUTPUTFILE=/dev/lpvi0 -'

>     if [ $# -eq 0 ]
>     then
>       $outcmd1 | $outcmd2
>     else
>       cat $* | $outcmd1 | $outcmd2
>     fi

### Problems

Since `/dev/lpi` can be opened only for exclusive use, if another job has it open (engine_ctl_sparc or another Ghostscript are the most likely candidates), Ghostscript stops with "Error: /invalidfileaccess in --.outputpage--"

In case of common printer problems like being out of paper, a warning describing the reason is printed to stdout. The driver tries access again each five seconds. Due to a problem with the device driver (in the kernel) the reason for printer failure isn't always reported correctly to the program. This is the case, for instance, if you open the top cover (error E5 on the printer's display). Look at the display on the printer itself if a "Printer problem with unknown reason" is reported. Fatal errors cause the print job to be terminated.

Note: there is some confusion whether the resolution setting should be the integers 300 and 400, or the symbolic constants DPI300 and DPI400 (defined in lpviio.h). Ghostscript releases have had it both ways. It is currently the latter. However, INOUE Namihiko reports (in bug #215256) that the former works better for him. If anyone has a definitive answer, please let us know.

## Apple dot matrix printer

This section was contributed by Mark Wedel <master@cats.ucsc.edu>.

The Apple Dot Matrix Printer (DMP) was a parallel predecessor to the Imagewriter printer. As far as I know, Imagewriter commands are a superset of the Dot Matrix printer's, so the driver should generate output that can be printed on Imagewriters.

To print images, the driver sets the printer for unidirectional printing and 15 characters per inch (cpi), or 120dpi. It sets the line feed to 1/9 inch. When finished, it sets the printer to bidirectional printing, 1/8-inch line feeds, and 12 cpi. There appears to be no way to reset the printer to initial values.

This code does not set for 8-bit characters (which is required). It also assumes that carriage return-newline is needed, and not just carriage return. These are all switch settings on the DMP, and I have configured them for 8-bit data and carriage return exclusively. Ensure that the Unix printer daemon handles 8-bit (binary) data properly; in my SunOS 4.1.1 `printcap` file the string "`ms=pass8,-opost`" works fine for this.

Finally, you can search `devdemp.c` for "`Init`" and "`Reset`" to find the strings that initialize the printer and reset things when finished, and change them to meet your needs.

## Special and Test devices

The devices in this section are intended primarily for testing. They may be interesting as code examples, as well.

### Raw 'bit' devices

There are a collection of 'bit' devices that don't do any special formatting but output 'raw' binary data for the page images. These are used for benchmarking but can also be useful when you want to directly access the raster data.

The raw devices are `bit bitrgb bitcmyk`.

### Bounding box output

There is a special `bbox` "device" that just prints the bounding box of each page. You select it in the usual way:

> `gs -dSAFER -dNOPAUSE -dBATCH -sDEVICE=bbox`

It prints the output in a format like this:

>     %%BoundingBox: 14 37 570 719
>     %%HiResBoundingBox: 14.308066 37.547999 569.495061 718.319158

Currently, it always prints the bounding box on `stderr`; eventually, it should also recognize `-sOutputFile=`.

By default, white objects don't contribute to the bounding box because many files fill the whole page with white before drawing other objects. This can be changed by:

> `<< /WhiteIsOpaque true >> setpagedevice`

Note that this device, like other devices, has a resolution and a (maximum) page size. As for other devices, the product (resolution x page size) is limited to approximately 500K pixels. By default, the resolution is 4000 DPI and the maximum page size is approximately 125", or approximately 9000 default (1/72") user coordinate units. If you need to measure larger pages than this, you must reset both the resolution and the page size in pixels, e.g.,

> `gs -dNOPAUSE -dBATCH -sDEVICE=bbox -r100 -g500000x500000`

### Permutation (DeviceN color model)

With no additional parameters, the device named "permute" looks to Ghostscript like a standard CMYK contone device, and outputs a PPM file, using a simple CMYK->RGB transform. This should be the baseline for regression testing.

With the addition of `-dPermute=1`, the internal behavior changes somewhat, but in most cases the resulting rendered file should be the same. In this mode, the color model becomes "DeviceN" rather than "DeviceCMYK", the number of components goes to six, and the color model is considered to be the (yellow, cyan, cyan, magenta, 0, black) tuple. This is what's rendered into the memory buffer. Finally, on conversion to RGB for output, the colors are permuted back.

As such, this code should check that all imaging code paths are 64-bit clean. Additionally, it should find incorrect code that assumes that the color model is one of DeviceGray, DeviceRGB, or DeviceCMYK.

Currently, the code has the limitation of 8-bit continuous tone rendering only. An enhancement to do halftones is planned as well. Note, however, that when testing permuted halftones for consistency, it is important to permute the planes of the default halftone accordingly, and that any file which sets halftones explicitly will fail a consistency check.

### spotcmyk (DeviceN color model)

The `spotcmyk` device was created for debugging and testing of the DeviceN extensions to Ghostscript that were released in version 8.0. There are also another device (`devicen`) in the same source file. It were created for testing however it are not actually useful except as example code.

The `spotcmyk` device was also designed to provide example code for a device which supports spot colors. Spot colors need to be specified prior to opening the first page. This can be done via adding the following to the command line: `-c "<< /SeparationColorNames [ /Name1 /Name2 ] >> setpagedevice" -f`.

The `spotcmyk` device produces a binary data file (similar to the bitcmyk device) for the CMYK data. This data file has the name specified by the "OutputFile" parameter. The device also produces a binary data file (similar to the bitmono device) for each spot color plane. These data files have the name specified by the "OutputFile" parameter with "sn" appended to the end (where "n" is the spot color number 0 to 12)".

After the `spotcmyk` device produces the binary data files, the files are read and PCX format versions of these files are created with ".pcx" appended to the binary source file name.

If the the `spotcmyk` is being used with three spot colors and the "OutputFile" parameter is `xxx` then the following files would be created by the device:

>     xxx - binary CMYK data
>     xxxs0 - binary data for first spot color
>     xxxs1 - binary data for second spot color
>     xxxs2 - binary data for third spot color
>     xxx.pcx - CMYK data in PCX format
>     xxxs0.pcx - first spot color in PCX format
>     xxxs1.pcx - second spot color in PCX format
>     xxxs2.pcx - third spot color in PCX format

The `spotcmyk` device has the creation of the binary data files separated from the creation of the PCX files since the source file is intended as example code and many people may not be interested in the PCX format. The PCX format was chosen because it was simple to implement from preexisting code and viewers are available. The PCX format does have the disadvantage that most of those viewers are on Windows.

### XCF (DeviceN color model)

The XCF file format is the native image format for the GIMP program. This format is currently supported by two devices: `xcfrgb` and `xcfcmyk`.

> We have been warned by the people supporting the GIMP program that they reserve the right to change the XCF format at anytime and thus these devices may become invalid. They are being included in the documentation because we have received some questions about these devices do.

The XCF devices were created for testing of the DeviceN extensions to Ghostscript which were released in version 8.0.

The `xcfrgb` device uses a DeviceRGB process color model and creates a normal XCF file.

The `xcfcmyk` device was created as a means of viewing spot colors for those users that do not have access to either Photoshop (see the PSD devices) or a PCX viewer (see the `spotcmyk` device).

The `xcfcmyk` device starts by using a DeviceCMYK process color model. The DeviceCMYK process color model allows the `xcfcmyk` device to also support spot colors. Spot colors need to be specified prior to opening the first page. This can be done via adding the following to the command line: `-c "<< /SeparationColorNames [ /Name1 /Name2 ] >> setpagedevice" -f`.

After a page is complete, the `xcfcmyk` converts the CMYK image data into RGB for storing in the XCF output file. The XCF format does not currently support CMYK data directly. The spot color planes are converted into alpha channel planes. This is done because the XCF format does not currently support spot colors.

Copyright © 2000-2006 artofcode LLC. All rights reserved.

This software is provided AS-IS with no warranty, either express or implied. This software is distributed under license and may not be copied, modified or distributed except as expressly authorized under the terms of that license. Refer to licensing information at http://www.artifex.com/ or contact Artifex Software, Inc., 7 Mt. Lassen Drive - Suite A-134, San Rafael, CA 94903, U.S.A., +1(415)492-9861, for further information.

Ghostscript version 8.56, 14 March 2007